|  |  |  |  |
| --- | --- | --- | --- |
| Function | Command | Barcode | Remark |
|  | @SET |  |  |
| USB VCP COM | WN-W-L1001 |  | USB virtual serial port need to install the serial port (USB) driver can be normal use |
|  | @END |  |  |

按顺序扫描下方条码设置USB虚拟串口